|  |  |
| --- | --- |
| **Respirator Inspection Checklist** | |
| **Face piece** | No cracks, tears, or holes  No facemask distortion  No cracked or loose lenses or face shields |
| **Head straps** | No breaks or tears  No broken buckles |
| **Valves** | No residue or dirt, cracks, or tears in valve material |
| **Filters and cartridges** | NIOSH approved  Gaskets seat properly  No cracks or dents in housing  Proper cartridge for hazards |
| **Air supply systems** | Breathing-quality air is used  Supply hoses are in good condition  Hoses are properly connected  Settings on regulators and valves are correct |

\*This checklist represents a general overview of respirator inspection requirements. Always refer to the manufacturer’s user manual for more detailed information.